North Star Imaging, Inc.
CT Geometry summary

Computation date: 			2/18/2021 8:57:36 AM

Tracking:: 				12 points used, over 60 views

Geometry tool: 				5 mm - medium tool, Spacing [5.000000] mm ([0.19685] inches)

Detector pixel pitch: 			0.2x0.2 mm (0.00787x0.00787 inches)

Image modification: 			Rotate(270 degree)

Xray-source / Detector distance:		1551.314 mm (61.075 inches)
Rotation axis / Detector distance: 	1288.991 mm (50.748 inches)
Rotation axis / Xray-source distance: 	262.323 mm (10.328 inches)

Magnification: 				x5.91
Optimum voxel size: 			33.8 microns (0.001331 inches)
Geometric unsharpness:			x4.9
	5 micron focal spot will be 24.57 micron wide (0.12 pixels)

Rotation: 				Found Counter-Clockwise (CCW) rotation direction
Rotation axis: 				0.00121279557976508 -0.99999926456317 0
Rotation axis angle: 			-179.931 degree

Image center: 				(202.707, 238.36) mm  / (7.981, 9.384) inches

Images folder: 		Geometry
Starting image used: 			geom*.tif
  60 images, 6 degree step

radiographs "Radiographs-Pitt_5 per-FER-6_MIC\Pitt_5 per-FER-6_MIC-radio*.tif"
	0.25 degree angle step (assuming a full 360 degree acquisition)