North Star Imaging, Inc.
CT Geometry summary

Computation date: 			5/24/2021 2:17:26 PM

Tracking:: 				13 points used, over 60 views

Geometry tool: 				5 mm - medium tool, Spacing [5.000000] mm ([0.19685] inches)

Detector pixel pitch: 			0.2x0.2 mm (0.00787x0.00787 inches)

Image modification: 			Rotate(270 degree)

Xray-source / Detector distance:		1552.607 mm (61.126 inches)
Rotation axis / Detector distance: 	1280.496 mm (50.413 inches)
Rotation axis / Xray-source distance: 	272.111 mm (10.713 inches)

Magnification: 				x5.71
Optimum voxel size: 			35.1 microns (0.00138 inches)
Geometric unsharpness:			x4.7
	5 micron focal spot will be 23.53 micron wide (0.12 pixels)

Rotation: 				Found Counter-Clockwise (CCW) rotation direction
Rotation axis: 				0.00105520779236502 -0.999999443268103 0
Rotation axis angle: 			-179.94 degree

Image center: 				(202.372, 240.41) mm  / (7.967, 9.465) inches

Images folder: 		Geometry
Starting image used: 			geom*.tif
  60 images, 6 degree step

radiographs "Radiographs-Flex-1_30 per_6000_MIC\Flex-1_30 per_6000_MIC-radio*.tif"
	0.25 degree angle step (assuming a full 360 degree acquisition)