North Star Imaging, Inc.
CT Geometry summary

Computation date: 			5/24/2021 6:20:59 AM

Tracking:: 				12 points used, over 60 views

Geometry tool: 				5 mm - medium tool, Spacing [5.000000] mm ([0.19685] inches)

Detector pixel pitch: 			0.2x0.2 mm (0.00787x0.00787 inches)

Image modification: 			Rotate(270 degree)

Xray-source / Detector distance:		1551.789 mm (61.094 inches)
Rotation axis / Detector distance: 	1299.862 mm (51.176 inches)
Rotation axis / Xray-source distance: 	251.928 mm (9.918 inches)

Magnification: 				x6.16
Optimum voxel size: 			32.5 microns (0.001278 inches)
Geometric unsharpness:			x5.2
	5 micron focal spot will be 25.8 micron wide (0.13 pixels)

Rotation: 				Found Counter-Clockwise (CCW) rotation direction
Rotation axis: 				0.00102276571132879 -0.999999476975013 0
Rotation axis angle: 			-179.941 degree

Image center: 				(202.171, 238.363) mm  / (7.959, 9.384) inches

Images folder: 		Geometry
Starting image used: 			geom*.tif
  60 images, 6 degree step

radiographs "Radiographs-Neat-Class-H-3_MIC\Neat-Class-H-3_MIC-radio*.tif"
	0.25 degree angle step (assuming a full 360 degree acquisition)