North Star Imaging, Inc.
CT Geometry summary

Computation date: 			5/20/2021 3:24:28 PM

Tracking:: 				12 points used, over 60 views

Geometry tool: 				5 mm - medium tool, Spacing [5.000000] mm ([0.19685] inches)

Detector pixel pitch: 			0.2x0.2 mm (0.00787x0.00787 inches)

Image modification: 			Rotate(270 degree)

Xray-source / Detector distance:		1551.595 mm (61.086 inches)
Rotation axis / Detector distance: 	1309.684 mm (51.562 inches)
Rotation axis / Xray-source distance: 	241.911 mm (9.524 inches)

Magnification: 				x6.41
Optimum voxel size: 			31.2 microns (0.001228 inches)
Geometric unsharpness:			x5.4
	5 micron focal spot will be 27.07 micron wide (0.14 pixels)

Rotation: 				Found Counter-Clockwise (CCW) rotation direction
Rotation axis: 				0.00102504532711957 -0.999999474640901 0
Rotation axis angle: 			-179.941 degree

Image center: 				(202.212, 238.54) mm  / (7.961, 9.391) inches

Images folder: 		Geometry
Starting image used: 			geom*.tif
  60 images, 6 degree step

radiographs "Radiographs-Neat-Class-H-6_MIC\Neat-Class-H-6_MIC-radio*.tif"
	0.25 degree angle step (assuming a full 360 degree acquisition)