North Star Imaging, Inc.
CT Geometry summary

Computation date: 			9/1/2020 8:36:28 AM

Tracking:: 				12 points used, over 60 views

Geometry tool: 				5 mm - medium tool, Spacing [5.000000] mm ([0.19685] inches)

Detector pixel pitch: 			0.2x0.2 mm (0.00787x0.00787 inches)

Image modification: 			Rotate(270 degree)

Xray-source / Detector distance:		1559.633 mm (61.403 inches)
Rotation axis / Detector distance: 	1302.969 mm (51.298 inches)
Rotation axis / Xray-source distance: 	256.664 mm (10.105 inches)

Magnification: 				x6.08
Optimum voxel size: 			32.9 microns (0.001296 inches)
Geometric unsharpness:			x5.1
	5 micron focal spot will be 25.38 micron wide (0.13 pixels)

Rotation: 				Found Counter-Clockwise (CCW) rotation direction
Rotation axis: 				0.00106609977298513 -0.999999431715476 0
Rotation axis angle: 			-179.939 degree

Image center: 				(203.982, 237.272) mm  / (8.031, 9.341) inches

Images folder: 		Geometry
Starting image used: 			geom*.tif
  60 images, 6 degree step

radiographs "Radiographs-OSU_Cem_Neat-1_MIC\OSU_Cem_Neat-1_MIC-radio*.tif"
	0.25 degree angle step (assuming a full 360 degree acquisition)